# Static Call Graph for image ..\OBJ\LCD-SPI.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Mon Oct 07 12:42:53 2019

### Maximum Stack Usage = 576 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ rtp_test ⇒ Load_Drow_Dialog ⇒ GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FPU_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PVD_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - RCC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - Reset_Handler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f40_41xxx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TP_Adjust from touch.o(i.TP_Adjust) referenced from touch.o(.data)
  - TP_Init from touch.o(i.TP_Init) referenced from touch.o(.data)
  - TP_Scan from touch.o(i.TP_Scan) referenced from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART1_IRQHandler from usart.o(i.USART1_IRQHandler) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f40_41xxx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f40_41xxx.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> GBK_Show_StrMid

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> TP_Adjust

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> TP_Adjust

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> TP_Adjust

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cdcmple.o(.text), UNUSED)

  __aeabi_cdcmple (Thumb, 48 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> _double_epilogue
  - >> _dsqrt

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> _double_epilogue
  - >> _dsqrt

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsl
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> __hardfp_sqrt

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  Color_Test (Thumb, 222 bytes, Stack size 24 bytes, lcd.o(i.Color_Test))
  [Stack]

  - Max Depth = 284
  - Call Chain = Color_Test ⇒ Draw_Font16B ⇒ Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Draw_Font16B
  - >> LCD_Fill
  - >> Draw_Test
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> Demo_Menu

  Copy_HZK16 (Thumb, 60 bytes, Stack size 28 bytes, text.o(i.Copy_HZK16))
  [Stack]

  - Max Depth = 36
  - Call Chain = Copy_HZK16 ⇒ Copy_Mem
  [Calls]
  - >> Copy_Mem
  [Called By]
  - >> Get_HzMat

  Copy_HZK24 (Thumb, 64 bytes, Stack size 28 bytes, text.o(i.Copy_HZK24))
  [Stack]

  - Max Depth = 36
  - Call Chain = Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Copy_Mem
  [Called By]
  - >> Get_HzMat

  Copy_Mem (Thumb, 22 bytes, Stack size 8 bytes, text.o(i.Copy_Mem))
  [Stack]

  - Max Depth = 8
  - Call Chain = Copy_Mem
  [Called By]
  - >> Copy_HZK24
  - >> Copy_HZK16

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  Demo_Menu (Thumb, 174 bytes, Stack size 8 bytes, lcd.o(i.Demo_Menu))
  [Stack]

  - Max Depth = 528
  - Call Chain = Demo_Menu ⇒ GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> Show_Picture
  - >> Draw_Font24B
  - >> Draw_Font16B
  - >> Font_Test
  - >> DisplayButtonUp
  - >> Color_Test
  - >> delay_ms
  - >> LCD_Clear
  - >> GBK_LibFont_Test
  [Called By]
  - >> main

  DisplayButtonUp (Thumb, 126 bytes, Stack size 32 bytes, lcd.o(i.DisplayButtonUp))
  [Stack]

  - Max Depth = 108
  - Call Chain = DisplayButtonUp ⇒ LCD_DrawLine ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_DrawLine
  [Called By]
  - >> Demo_Menu

  DrawFontASC_GBK48B (Thumb, 50 bytes, Stack size 40 bytes, gbk_libdrive.o(i.DrawFontASC_GBK48B))
  [Stack]

  - Max Depth = 456
  - Call Chain = DrawFontASC_GBK48B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  [Called By]
  - >> GBK_LibFont_Test

  DrawFontASC_GBK64B (Thumb, 50 bytes, Stack size 40 bytes, gbk_libdrive.o(i.DrawFontASC_GBK64B))
  [Stack]

  - Max Depth = 456
  - Call Chain = DrawFontASC_GBK64B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  [Called By]
  - >> GBK_LibFont_Test

  DrawFont_GBK12B (Thumb, 50 bytes, Stack size 40 bytes, gbk_libdrive.o(i.DrawFont_GBK12B))
  [Stack]

  - Max Depth = 456
  - Call Chain = DrawFont_GBK12B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  [Called By]
  - >> GBK_LibFont_Test

  DrawFont_GBK16B (Thumb, 50 bytes, Stack size 40 bytes, gbk_libdrive.o(i.DrawFont_GBK16B))
  [Stack]

  - Max Depth = 456
  - Call Chain = DrawFont_GBK16B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  [Called By]
  - >> GBK_LibFont_Test
  - >> GBK_ReadID

  DrawFont_GBK32B (Thumb, 50 bytes, Stack size 40 bytes, gbk_libdrive.o(i.DrawFont_GBK32B))
  [Stack]

  - Max Depth = 456
  - Call Chain = DrawFont_GBK32B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  [Called By]
  - >> GBK_LibFont_Test

  Draw_Font16B (Thumb, 42 bytes, Stack size 40 bytes, text.o(i.Draw_Font16B))
  [Stack]

  - Max Depth = 260
  - Call Chain = Draw_Font16B ⇒ Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Show_Str
  [Called By]
  - >> Show_Picture
  - >> Font_Test
  - >> Color_Test
  - >> Demo_Menu

  Draw_Font24B (Thumb, 42 bytes, Stack size 40 bytes, text.o(i.Draw_Font24B))
  [Stack]

  - Max Depth = 260
  - Call Chain = Draw_Font24B ⇒ Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Show_Str
  [Called By]
  - >> Font_Test
  - >> Demo_Menu

  Draw_Test (Thumb, 110 bytes, Stack size 16 bytes, lcd.o(i.Draw_Test))
  [Stack]

  - Max Depth = 120
  - Call Chain = Draw_Test ⇒ LCD_DrawRectangle ⇒ LCD_DrawLine ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_Draw_Circle
  - >> LCD_DrawRectangle
  - >> LCD_DrawLine
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> Color_Test

  FontLib_Read (Thumb, 92 bytes, Stack size 24 bytes, gbk_libdrive.o(i.FontLib_Read))
  [Stack]

  - Max Depth = 48
  - Call Chain = FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GBK_delay
  - >> Font_SPI_WR
  [Called By]
  - >> GBK_ReadID
  - >> GBK_Lib_GetHz
  - >> GBK_GetASC_Point

  Font_SPI_WR (Thumb, 86 bytes, Stack size 24 bytes, gbk_libdrive.o(i.Font_SPI_WR))
  [Stack]

  - Max Depth = 24
  - Call Chain = Font_SPI_WR
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> FontLib_Read

  Font_Test (Thumb, 170 bytes, Stack size 16 bytes, lcd.o(i.Font_Test))
  [Stack]

  - Max Depth = 276
  - Call Chain = Font_Test ⇒ Draw_Font24B ⇒ Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Draw_Font24B
  - >> Draw_Font16B
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> Demo_Menu

  GBK_GetASC_Point (Thumb, 96 bytes, Stack size 8 bytes, gbk_libdrive.o(i.GBK_GetASC_Point))
  [Stack]

  - Max Depth = 56
  - Call Chain = GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> FontLib_Read
  [Called By]
  - >> GBK_ShowASCII

  GBK_LibFont_Test (Thumb, 306 bytes, Stack size 48 bytes, gbk_libdrive.o(i.GBK_LibFont_Test))
  [Stack]

  - Max Depth = 520
  - Call Chain = GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> delay_ms
  - >> LCD_Clear
  - >> GBK_Show_Str
  - >> GBK_Show_StrMid
  - >> DrawFont_GBK32B
  - >> DrawFont_GBK16B
  - >> DrawFont_GBK12B
  - >> DrawFontASC_GBK64B
  - >> DrawFontASC_GBK48B
  [Called By]
  - >> Demo_Menu
  - >> Load_Drow_Dialog

  GBK_Lib_GetHz (Thumb, 126 bytes, Stack size 8 bytes, gbk_libdrive.o(i.GBK_Lib_GetHz))
  [Stack]

  - Max Depth = 56
  - Call Chain = GBK_Lib_GetHz ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> FontLib_Read
  [Called By]
  - >> GBK_Show_Font

  GBK_Lib_Init (Thumb, 76 bytes, Stack size 24 bytes, gbk_libdrive.o(i.GBK_Lib_Init))
  [Stack]

  - Max Depth = 520
  - Call Chain = GBK_Lib_Init ⇒ GBK_ReadID ⇒ DrawFont_GBK16B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> GBK_ReadID
  [Called By]
  - >> main

  GBK_ReadID (Thumb, 134 bytes, Stack size 40 bytes, gbk_libdrive.o(i.GBK_ReadID))
  [Stack]

  - Max Depth = 496
  - Call Chain = GBK_ReadID ⇒ DrawFont_GBK16B ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> delay_ms
  - >> LCD_Clear
  - >> FontLib_Read
  - >> DrawFont_GBK16B
  [Called By]
  - >> GBK_Lib_Init

  GBK_ShowASCII (Thumb, 170 bytes, Stack size 296 bytes, gbk_libdrive.o(i.GBK_ShowASCII))
  [Stack]

  - Max Depth = 352
  - Call Chain = GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> LCD_Fast_DrawPoint
  - >> GBK_GetASC_Point
  [Called By]
  - >> GBK_Show_Str

  GBK_Show_Font (Thumb, 160 bytes, Stack size 168 bytes, gbk_libdrive.o(i.GBK_Show_Font))
  [Stack]

  - Max Depth = 224
  - Call Chain = GBK_Show_Font ⇒ GBK_Lib_GetHz ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> LCD_Fast_DrawPoint
  - >> GBK_Lib_GetHz
  [Called By]
  - >> GBK_Show_Str

  GBK_Show_Str (Thumb, 190 bytes, Stack size 64 bytes, gbk_libdrive.o(i.GBK_Show_Str))
  [Stack]

  - Max Depth = 416
  - Call Chain = GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Font
  - >> GBK_ShowASCII
  [Called By]
  - >> TP_Adjust
  - >> GBK_LibFont_Test
  - >> Load_Drow_Dialog
  - >> GBK_Show_StrMid
  - >> DrawFont_GBK32B
  - >> DrawFont_GBK16B
  - >> DrawFont_GBK12B
  - >> DrawFontASC_GBK64B
  - >> DrawFontASC_GBK48B

  GBK_Show_StrMid (Thumb, 100 bytes, Stack size 56 bytes, gbk_libdrive.o(i.GBK_Show_StrMid))
  [Stack]

  - Max Depth = 472
  - Call Chain = GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> GBK_Show_Str
  - >> strlen
  [Called By]
  - >> GBK_LibFont_Test

  GBK_delay (Thumb, 24 bytes, Stack size 0 bytes, gbk_libdrive.o(i.GBK_delay))
  [Called By]

  - >> FontLib_Read

  GPIO_Init (Thumb, 124 bytes, Stack size 24 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> SPI2_Init
  - >> LCD_GPIO_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> LED_Init
  - >> KEY_Init
  - >> GBK_Lib_Init
  - >> TP_Init
  - >> SPI3_Init

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> SPI2_Init
  - >> uart_init
  - >> SPI3_Init

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> KEY_Scan
  - >> Font_SPI_WR

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> Font_SPI_WR
  - >> FontLib_Read

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LED_Init
  - >> GBK_Lib_Init
  - >> Font_SPI_WR
  - >> FontLib_Read

  Get_HzMat (Thumb, 80 bytes, Stack size 8 bytes, text.o(i.Get_HzMat))
  [Stack]

  - Max Depth = 44
  - Call Chain = Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Copy_HZK24
  - >> Copy_HZK16
  [Called By]
  - >> Show_Font

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  KEY_Init (Thumb, 40 bytes, Stack size 16 bytes, key.o(i.KEY_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Scan (Thumb, 72 bytes, Stack size 16 bytes, key.o(i.KEY_Scan))
  [Stack]

  - Max Depth = 32
  - Call Chain = KEY_Scan ⇒ delay_ms
  [Calls]
  - >> delay_ms
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> rtp_test

  LCD_Clear (Thumb, 54 bytes, Stack size 20 bytes, lcd.o(i.LCD_Clear))
  [Stack]

  - Max Depth = 52
  - Call Chain = LCD_Clear ⇒ LCD_Set_Window ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA16
  - >> LCD_Set_Window
  - >> LCD_SetCursor
  [Called By]
  - >> Show_Picture
  - >> Font_Test
  - >> Draw_Test
  - >> Color_Test
  - >> TP_Adjust
  - >> LCD_Init
  - >> GBK_LibFont_Test
  - >> Demo_Menu
  - >> rtp_test
  - >> main
  - >> TP_Init
  - >> GBK_ReadID

  LCD_Display_Dir (Thumb, 174 bytes, Stack size 20 bytes, lcd.o(i.LCD_Display_Dir))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_Display_Dir ⇒ LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA16
  - >> LCD_Scan_Dir
  [Called By]
  - >> LCD_Init

  LCD_DrawLine (Thumb, 154 bytes, Stack size 48 bytes, lcd.o(i.LCD_DrawLine))
  [Stack]

  - Max Depth = 76
  - Call Chain = LCD_DrawLine ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> LCD_DrawRectangle
  - >> Draw_Test
  - >> DisplayButtonUp
  - >> TP_Drow_Touch_Point

  LCD_DrawPoint (Thumb, 22 bytes, Stack size 4 bytes, lcd.o(i.LCD_DrawPoint))
  [Stack]

  - Max Depth = 28
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA16
  - >> LCD_SetCursor
  [Called By]
  - >> TP_Draw_Big_Point
  - >> TP_Drow_Touch_Point

  LCD_DrawRectangle (Thumb, 74 bytes, Stack size 28 bytes, lcd.o(i.LCD_DrawRectangle))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_DrawRectangle ⇒ LCD_DrawLine ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_DrawLine
  [Called By]
  - >> Draw_Test

  LCD_Draw_Circle (Thumb, 200 bytes, Stack size 60 bytes, lcd.o(i.LCD_Draw_Circle))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_Draw_Circle ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> Draw_Test
  - >> TP_Drow_Touch_Point

  LCD_Fast_DrawPoint (Thumb, 50 bytes, Stack size 20 bytes, lcd.o(i.LCD_Fast_DrawPoint))
  [Stack]

  - Max Depth = 28
  - Call Chain = LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA16
  [Called By]
  - >> Show_Font
  - >> LCD_ShowChar
  - >> LCD_Draw_Circle
  - >> LCD_DrawLine
  - >> GBK_Show_Font
  - >> GBK_ShowASCII

  LCD_Fill (Thumb, 140 bytes, Stack size 28 bytes, lcd.o(i.LCD_Fill))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_Fill ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_REG
  - >> LCD_WR_DATA16
  [Called By]
  - >> Color_Test

  LCD_GPIO_Init (Thumb, 92 bytes, Stack size 24 bytes, lcd.o(i.LCD_GPIO_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_GPIO_Init ⇒ SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI2_Init
  - >> LCD_HardwareRest
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> LCD_Init

  LCD_HardwareRest (Thumb, 32 bytes, Stack size 8 bytes, lcd.o(i.LCD_HardwareRest))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_HardwareRest ⇒ delay_ms
  [Calls]
  - >> delay_ms
  [Called By]
  - >> LCD_GPIO_Init

  LCD_Init (Thumb, 532 bytes, Stack size 8 bytes, lcd.o(i.LCD_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_Init ⇒ LCD_GPIO_Init ⇒ SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA8
  - >> LCD_SoftRest
  - >> LCD_GPIO_Init
  - >> LCD_Display_Dir
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> main

  LCD_Pow (Thumb, 16 bytes, Stack size 0 bytes, lcd.o(i.LCD_Pow))
  [Called By]

  - >> LCD_ShowNum

  LCD_Scan_Dir (Thumb, 54 bytes, Stack size 0 bytes, lcd.o(i.LCD_Scan_Dir))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_Display_Dir

  LCD_SetCursor (Thumb, 36 bytes, Stack size 16 bytes, lcd.o(i.LCD_SetCursor))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetCursor ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA16
  [Called By]
  - >> LCD_DrawPoint
  - >> LCD_Clear

  LCD_Set_Window (Thumb, 68 bytes, Stack size 24 bytes, lcd.o(i.LCD_Set_Window))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_Set_Window ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA16
  [Called By]
  - >> Show_Picture
  - >> LCD_Clear

  LCD_ShowChar (Thumb, 200 bytes, Stack size 40 bytes, lcd.o(i.LCD_ShowChar))
  [Stack]

  - Max Depth = 68
  - Call Chain = LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> Show_Str
  - >> LCD_ShowNum
  - >> LCD_ShowString

  LCD_ShowNum (Thumb, 124 bytes, Stack size 60 bytes, lcd.o(i.LCD_ShowNum))
  [Stack]

  - Max Depth = 128
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_ShowChar
  - >> LCD_Pow
  [Called By]
  - >> TP_Adj_Info_Show

  LCD_ShowString (Thumb, 84 bytes, Stack size 44 bytes, lcd.o(i.LCD_ShowString))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adjust
  - >> main
  - >> Load_Drow_Dialog
  - >> TP_Adj_Info_Show

  LCD_SoftRest (Thumb, 18 bytes, Stack size 8 bytes, lcd.o(i.LCD_SoftRest))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SoftRest ⇒ delay_ms
  [Calls]
  - >> LCD_WR_REG
  - >> delay_ms
  [Called By]
  - >> LCD_Init

  LCD_WR_DATA16 (Thumb, 38 bytes, Stack size 8 bytes, lcd.o(i.LCD_WR_DATA16))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_DATA16
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_SetCursor
  - >> LCD_Fill
  - >> LCD_Fast_DrawPoint
  - >> LCD_DrawPoint
  - >> LCD_Display_Dir
  - >> LCD_Clear

  LCD_WR_DATA8 (Thumb, 28 bytes, Stack size 4 bytes, lcd.o(i.LCD_WR_DATA8))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_WR_DATA8
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> Show_Picture
  - >> LCD_WriteReg
  - >> LCD_Init

  LCD_WR_REG (Thumb, 30 bytes, Stack size 4 bytes, lcd.o(i.LCD_WR_REG))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_WR_REG
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> LCD_WriteReg
  - >> LCD_WriteRAM_Prepare
  - >> LCD_SoftRest
  - >> LCD_Set_Window
  - >> LCD_SetCursor
  - >> LCD_Fill
  - >> LCD_Fast_DrawPoint
  - >> LCD_Display_Dir
  - >> LCD_Init

  LCD_WriteRAM_Prepare (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(i.LCD_WriteRAM_Prepare))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_WriteRAM_Prepare ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WR_REG
  [Called By]
  - >> Show_Picture
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> LCD_Clear

  LCD_WriteReg (Thumb, 18 bytes, Stack size 8 bytes, lcd.o(i.LCD_WriteReg))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_WriteReg ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_DATA8
  [Called By]
  - >> LCD_Scan_Dir

  LED_Init (Thumb, 58 bytes, Stack size 24 bytes, led.o(i.LED_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  Load_Drow_Dialog (Thumb, 108 bytes, Stack size 40 bytes, main.o(i.Load_Drow_Dialog))
  [Stack]

  - Max Depth = 560
  - Call Chain = Load_Drow_Dialog ⇒ GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> LCD_ShowString
  - >> GBK_Show_Str
  - >> GBK_LibFont_Test
  [Called By]
  - >> rtp_test

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  NVIC_Init (Thumb, 98 bytes, Stack size 12 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> main

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> SPI2_Init
  - >> LCD_GPIO_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> LED_Init
  - >> KEY_Init
  - >> GBK_Lib_Init
  - >> TP_Init
  - >> SPI3_Init

  RCC_APB1PeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> SPI2_Init
  - >> SPI3_Init

  RCC_APB1PeriphResetCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> SPI2_Init
  - >> SPI3_Init

  RCC_APB2PeriphClockCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> uart_init

  RCC_GetClocksFreq (Thumb, 148 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  SPI2_Init (Thumb, 174 bytes, Stack size 56 bytes, lcd.o(i.SPI2_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> SPI2_ReadWriteByte
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> LCD_GPIO_Init

  SPI2_ReadWriteByte (Thumb, 26 bytes, Stack size 0 bytes, lcd.o(i.SPI2_ReadWriteByte))
  [Called By]

  - >> SPI2_Init
  - >> LCD_WR_REG
  - >> LCD_WR_DATA8
  - >> LCD_WR_DATA16

  SPI3_Init (Thumb, 182 bytes, Stack size 56 bytes, w25qxx.o(i.SPI3_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = SPI3_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Init

  SPI3_ReadWriteByte (Thumb, 26 bytes, Stack size 0 bytes, w25qxx.o(i.SPI3_ReadWriteByte))
  [Called By]

  - >> W25QXX_ReadID
  - >> W25QXX_Write_Page
  - >> W25QXX_Write_Enable
  - >> W25QXX_ReadSR
  - >> W25QXX_Read
  - >> W25QXX_Erase_Sector
  - >> SPI3_Init

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(i.SPI_Cmd))
  [Called By]

  - >> SPI2_Init
  - >> SPI3_Init

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f4xx_spi.o(i.SPI_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI2_Init
  - >> SPI3_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  Show_Font (Thumb, 164 bytes, Stack size 112 bytes, text.o(i.Show_Font))
  [Stack]

  - Max Depth = 156
  - Call Chain = Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Get_HzMat
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> Show_Str

  Show_Picture (Thumb, 104 bytes, Stack size 32 bytes, dis_picture.o(i.Show_Picture))
  [Stack]

  - Max Depth = 292
  - Call Chain = Show_Picture ⇒ Draw_Font16B ⇒ Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Draw_Font16B
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA8
  - >> LCD_Set_Window
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> Demo_Menu

  Show_Str (Thumb, 180 bytes, Stack size 64 bytes, text.o(i.Show_Str))
  [Stack]

  - Max Depth = 220
  - Call Chain = Show_Str ⇒ Show_Font ⇒ Get_HzMat ⇒ Copy_HZK24 ⇒ Copy_Mem
  [Calls]
  - >> Show_Font
  - >> LCD_ShowChar
  [Called By]
  - >> Draw_Font24B
  - >> Draw_Font16B

  SysTick_CLKSourceConfig (Thumb, 28 bytes, Stack size 0 bytes, misc.o(i.SysTick_CLKSourceConfig))
  [Called By]

  - >> delay_init

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(.text)

  TP_Adj_Info_Show (Thumb, 360 bytes, Stack size 64 bytes, touch.o(i.TP_Adj_Info_Show))
  [Stack]

  - Max Depth = 192
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_ShowNum
  - >> LCD_ShowString
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 1656 bytes, Stack size 120 bytes, touch.o(i.TP_Adjust))
  [Stack]

  - Max Depth = 536
  - Call Chain = TP_Adjust ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> delay_ms
  - >> LCD_ShowString
  - >> LCD_Clear
  - >> GBK_Show_Str
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_d2uiz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> TP_Save_Adjdata
  - >> TP_Get_Adjdata
  - >> TP_Drow_Touch_Point
  - >> TP_Adj_Info_Show
  - >> __hardfp_sqrt
  [Called By]
  - >> rtp_test
  - >> TP_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Draw_Big_Point (Thumb, 50 bytes, Stack size 16 bytes, touch.o(i.TP_Draw_Big_Point))
  [Stack]

  - Max Depth = 44
  - Call Chain = TP_Draw_Big_Point ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> rtp_test

  TP_Drow_Touch_Point (Thumb, 126 bytes, Stack size 32 bytes, touch.o(i.TP_Drow_Touch_Point))
  [Stack]

  - Max Depth = 120
  - Call Chain = TP_Drow_Touch_Point ⇒ LCD_Draw_Circle ⇒ LCD_Fast_DrawPoint ⇒ LCD_WR_DATA16
  [Calls]
  - >> LCD_Draw_Circle
  - >> LCD_DrawPoint
  - >> LCD_DrawLine
  [Called By]
  - >> TP_Adjust

  TP_Get_Adjdata (Thumb, 126 bytes, Stack size 32 bytes, touch.o(i.TP_Get_Adjdata))
  [Stack]

  - Max Depth = 48
  - Call Chain = TP_Get_Adjdata ⇒ W25QXX_Read
  [Calls]
  - >> W25QXX_Read
  [Called By]
  - >> TP_Adjust
  - >> TP_Init

  TP_Init (Thumb, 114 bytes, Stack size 24 bytes, touch.o(i.TP_Init))
  [Stack]

  - Max Depth = 560
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> TP_Adjust
  - >> LCD_Clear
  - >> TP_Read_XY
  - >> TP_Get_Adjdata
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Read_AD (Thumb, 110 bytes, Stack size 32 bytes, touch.o(i.TP_Read_AD))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 98 bytes, Stack size 32 bytes, touch.o(i.TP_Read_XOY))
  [Stack]

  - Max Depth = 88
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 34 bytes, Stack size 24 bytes, touch.o(i.TP_Read_XY))
  [Stack]

  - Max Depth = 112
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Read_XY2
  - >> TP_Init

  TP_Read_XY2 (Thumb, 134 bytes, Stack size 40 bytes, touch.o(i.TP_Read_XY2))
  [Stack]

  - Max Depth = 152
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Save_Adjdata (Thumb, 104 bytes, Stack size 32 bytes, touch.o(i.TP_Save_Adjdata))
  [Stack]

  - Max Depth = 124
  - Call Chain = TP_Save_Adjdata ⇒ W25QXX_Write ⇒ W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR
  [Calls]
  - >> W25QXX_Write
  [Called By]
  - >> TP_Adjust

  TP_Scan (Thumb, 168 bytes, Stack size 8 bytes, touch.o(i.TP_Scan))
  [Stack]

  - Max Depth = 160
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XY2
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Write_Byte (Thumb, 58 bytes, Stack size 24 bytes, touch.o(i.TP_Write_Byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = TP_Write_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> TP_Read_AD

  USART1_IRQHandler (Thumb, 92 bytes, Stack size 16 bytes, usart.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  USART_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_ClearFlag))
  [Called By]

  - >> uart_init

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_Cmd))
  [Called By]

  - >> uart_init

  USART_GetITStatus (Thumb, 64 bytes, Stack size 16 bytes, stm32f4xx_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_Init (Thumb, 180 bytes, Stack size 32 bytes, stm32f4xx_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  W25QXX_Erase_Sector (Thumb, 66 bytes, Stack size 8 bytes, w25qxx.o(i.W25QXX_Erase_Sector))
  [Stack]

  - Max Depth = 24
  - Call Chain = W25QXX_Erase_Sector ⇒ delay_ms
  [Calls]
  - >> delay_ms
  - >> W25QXX_Write_Enable
  - >> W25QXX_Wait_Busy
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Write

  W25QXX_Init (Thumb, 64 bytes, Stack size 16 bytes, w25qxx.o(i.W25QXX_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = W25QXX_Init ⇒ SPI3_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> W25QXX_ReadID
  - >> SPI3_Init
  [Called By]
  - >> main

  W25QXX_Read (Thumb, 72 bytes, Stack size 16 bytes, w25qxx.o(i.W25QXX_Read))
  [Stack]

  - Max Depth = 16
  - Call Chain = W25QXX_Read
  [Calls]
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> TP_Get_Adjdata
  - >> W25QXX_Write

  W25QXX_ReadID (Thumb, 56 bytes, Stack size 8 bytes, w25qxx.o(i.W25QXX_ReadID))
  [Stack]

  - Max Depth = 8
  - Call Chain = W25QXX_ReadID
  [Calls]
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Init
  - >> main

  W25QXX_ReadSR (Thumb, 26 bytes, Stack size 4 bytes, w25qxx.o(i.W25QXX_ReadSR))
  [Stack]

  - Max Depth = 4
  - Call Chain = W25QXX_ReadSR
  [Calls]
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Wait_Busy

  W25QXX_Wait_Busy (Thumb, 12 bytes, Stack size 4 bytes, w25qxx.o(i.W25QXX_Wait_Busy))
  [Stack]

  - Max Depth = 8
  - Call Chain = W25QXX_Wait_Busy ⇒ W25QXX_ReadSR
  [Calls]
  - >> W25QXX_ReadSR
  [Called By]
  - >> W25QXX_Write_Page
  - >> W25QXX_Erase_Sector

  W25QXX_Write (Thumb, 158 bytes, Stack size 40 bytes, w25qxx.o(i.W25QXX_Write))
  [Stack]

  - Max Depth = 92
  - Call Chain = W25QXX_Write ⇒ W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR
  [Calls]
  - >> W25QXX_Write_NoCheck
  - >> W25QXX_Read
  - >> W25QXX_Erase_Sector
  [Called By]
  - >> TP_Save_Adjdata

  W25QXX_Write_Enable (Thumb, 20 bytes, Stack size 4 bytes, w25qxx.o(i.W25QXX_Write_Enable))
  [Stack]

  - Max Depth = 4
  - Call Chain = W25QXX_Write_Enable
  [Calls]
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Write_Page
  - >> W25QXX_Erase_Sector

  W25QXX_Write_NoCheck (Thumb, 62 bytes, Stack size 24 bytes, w25qxx.o(i.W25QXX_Write_NoCheck))
  [Stack]

  - Max Depth = 52
  - Call Chain = W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR
  [Calls]
  - >> W25QXX_Write_Page
  [Called By]
  - >> W25QXX_Write

  W25QXX_Write_Page (Thumb, 80 bytes, Stack size 20 bytes, w25qxx.o(i.W25QXX_Write_Page))
  [Stack]

  - Max Depth = 28
  - Call Chain = W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR
  [Calls]
  - >> W25QXX_Write_Enable
  - >> W25QXX_Wait_Busy
  - >> SPI3_ReadWriteByte
  [Called By]
  - >> W25QXX_Write_NoCheck

  __hardfp_sqrt (Thumb, 122 bytes, Stack size 32 bytes, sqrt.o(i.__hardfp_sqrt))
  [Stack]

  - Max Depth = 72
  - Call Chain = __hardfp_sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> __hardfp_sqrt

  delay_init (Thumb, 38 bytes, Stack size 8 bytes, delay.o(i.delay_init))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_ms (Thumb, 50 bytes, Stack size 16 bytes, delay.o(i.delay_ms))
  [Stack]

  - Max Depth = 16
  - Call Chain = delay_ms
  [Calls]
  - >> delay_xms
  [Called By]
  - >> Show_Picture
  - >> LCD_SoftRest
  - >> LCD_HardwareRest
  - >> Font_Test
  - >> Draw_Test
  - >> Color_Test
  - >> TP_Adjust
  - >> LCD_Init
  - >> KEY_Scan
  - >> GBK_LibFont_Test
  - >> Demo_Menu
  - >> rtp_test
  - >> main
  - >> W25QXX_Erase_Sector
  - >> GBK_ReadID

  delay_us (Thumb, 46 bytes, Stack size 0 bytes, delay.o(i.delay_us))
  [Called By]

  - >> TP_Write_Byte
  - >> TP_Read_AD

  delay_xms (Thumb, 46 bytes, Stack size 0 bytes, delay.o(i.delay_xms))
  [Called By]

  - >> delay_ms

  main (Thumb, 202 bytes, Stack size 16 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 576
  - Call Chain = main ⇒ rtp_test ⇒ Load_Drow_Dialog ⇒ GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> uart_init
  - >> delay_ms
  - >> delay_init
  - >> W25QXX_ReadID
  - >> W25QXX_Init
  - >> NVIC_PriorityGroupConfig
  - >> LED_Init
  - >> LCD_ShowString
  - >> LCD_Init
  - >> LCD_Clear
  - >> KEY_Init
  - >> GBK_Lib_Init
  - >> Demo_Menu
  - >> rtp_test
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  rtp_test (Thumb, 142 bytes, Stack size 0 bytes, main.o(i.rtp_test))
  [Stack]

  - Max Depth = 560
  - Call Chain = rtp_test ⇒ Load_Drow_Dialog ⇒ GBK_LibFont_Test ⇒ GBK_Show_StrMid ⇒ GBK_Show_Str ⇒ GBK_ShowASCII ⇒ GBK_GetASC_Point ⇒ FontLib_Read ⇒ Font_SPI_WR
  [Calls]
  - >> delay_ms
  - >> TP_Draw_Big_Point
  - >> TP_Adjust
  - >> LCD_Clear
  - >> KEY_Scan
  - >> Load_Drow_Dialog
  [Called By]
  - >> main

  uart_init (Thumb, 172 bytes, Stack size 48 bytes, usart.o(i.uart_init))
  [Stack]

  - Max Depth = 96
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_ClearFlag
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  ### Local Symbols

  SetSysClock (Thumb, 168 bytes, Stack size 12 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols